ALGO 8180 G2 Configuration Example

Algo 8180 G2 is a good example of a manually configured SIP device useful as a loud ringer or external paging device (loud speaker).

Create a manual configured extension for use as a ringer, and as a paging extension. Two different extensions and uses.

Access the Algo's web interface using HTTPS and the device IP address. Find the IP address on your DHCP server and/or follow the Algo instructions.

Use the IP address of the Hello Hub as your SIP Server for both accounts.

Use the extension # as the login ID, and copy the password from the Hello Hub Extension Page.

Click 'Save' and test from other phones.

ring-u portal screen example

Matching ALGO 8180 G2 config screen example