ALGO 8180 Manual Config Example

Algo 8180 G2 is a good example of a manually configured SIP device useful as a loud ringer or external paging device (loud speaker). Create a manual configured extension for use as a ringer, and as a paging extension. This is 2 extensions per Algo 8180 G2 IF you want both “ringer only” and “PA”. There is a configuration screen on the ALGO for both accounts.

ring-u portal screen example

ALGO 8180 G2 config screen example