Ubiquiti UDM Pro

Advanced Settings for Dream Machine Pro (UDM Pro).

Search for SIP or Timeout. Adjust as below.

Under Firewall Connection Tracking (bottom of below image), make sure that SIP is not enabled. If there is a gray box showing SIP, that means it is enabled and you must click the X to dismiss/disable it.

Timeout should be set to a number greater that 600 seconds. 620 is recommended as our phones use 600.